**Shutter Control**

Nextion:

2 Buttons – “+” and “–“ to increase or decrease time setting

1 field – showing the time set

Button 1:

-Activating the relay on pin A5 for the time chosen via Nextion

Button 2:

-Activating the relay for as long as the button is pressed

Times to choose from / to scroll through:

|  |  |  |
| --- | --- | --- |
| Display | ms | s |
| 1/60 | 16,67 | 0,01667 |
| 1/30 | 33,33 | 0,03333 |
| 1/15 | 66,67 | 0,06667 |
| 1/8 | 125 | 0,125 |
| 1/4 | 250 | 0,25 |
| 1/2 | 500 | 0,5 |
| 1 | 1000 | 1 |
| 2 |  | 2 |
| 3 |  | 3 |
| 4 |  | 4 |
| … |  | … |
| 118 |  | 118 |
| 119 |  | 119 |
| 120 |  | 120 |